+ +

I’m confused by the ddr things. How come D7 is random? You never said what cmp.b did. How did you multiply by 78? What’s bpl dude?

How long is the delay time?

+ +

00 load from address 0 01 load from address 1 . . 1F load from address 1F (31) 20 write to address 0 . . 3F write to address 1F 40 add last two numbers 41 shift right once FF go back to the beginning